|  |  |  |
| --- | --- | --- |
| **S. No.** | **Description of Work** | **Quantity (Estimate)** |
| 1. | 1/3” color sony/equivalent CCD 5-10m IR Number Plate Capture Camera, 540 TVL, IP65 rated, 12 V DC power Supply | 2 Nos |
| 2.  | 1/3” Sony/equivalent OSD, C Mount Day & Night Camera, Horizontal resolution: 540 TV Lines, Min. Illumination: 0.1 Lux with 3.5 to 8 mm verifocal auto Iris Lens, Outdoor housing and Mounting Bracket | 2 Nos |
| 3.  | 4 Ch power supply for cameras | 1 No. |
| 4. | 20” TFT Monitor | 1 No. |
| 5.  | 4 Ch Standalone DVR, H.264 Compression, TCP/IP, CMS  | 1 No. |
| 6.  | Supply and Laying of power cable  | 100 m |
| 7. | CCTV Special Cable for perfect Video | 100 m |
| 8. | PVC conduit: ISI Mark 1” White | 100 m |
| 9. | Mounting poles for the Number Plate capture cameras/Day & Night Cameras (For both directions) 15” height, 6” diameter , GI Pipe | 1 No. |
| 10. | Wall Mounted Iron Grilled DVR box | 1 No. |
| 11. | Special Surveillance HDD (1 TB HDD) | 1 No. |
| 12. | Viewing Software | Single Site |
| 13. | Installation, testing and Commissioning Charges of CCTV System including various cameras, TFT, DVR, Viewing Software, DVR Box, Poles and other components/parts  | Single Site  |
| 14. | PVC conduit based Wire laying and installation charges per running meter | Single site |
|  |  |  |

**Annexure – “A-1”**

**Note:**

1. In addition to above, the offer should also mention Annual Maintenance Contract after the expiry of warranty period for single site.
2. The offer should also contain the quoted rate for 8-Channel, 16-Channel and 32-Channel Power Supply, Standalone DVRs and DVR boxes.
3. Wire laying and installation charges has to be quoted per running meter, however, the payment will be made as per actual.
4. Installation, testing and commissioning Charges of CCTV System including various cameras, TFT, DVR, Viewing Software, DVR Box, Poles and other components/parts